**PERMIT TEST**

1. The color of clearance lamps on the front of a vehicle must be
2. White
3. **Amber**
4. Green
5. Red
6. When backing a large truck you should
	1. Depend only on your rearview mirror
	2. Sound horn to clear way and back very slowly
	3. **Have someone guide you**
	4. Look straight ahead so you can back straight
7. Every trailer must have how many reflections on the rear?
8. **Two**
9. None
10. One
11. Three
12. When turning right with a long vehicle or combination truck-trailer, if it is impossible to stay in the proper lane, you should
13. Approach the corner 12 feet from the curb or right edge of roadway, then turn into the right-hand lane
14. **Approach the corner about 4 feet from the curb or right edge of the roadway, then if necessary complete turn in center of street entered.**
15. Permit rear wheels to run over curb if no obstruction is there.
16. Approach the corner in center of street then turn into right-hand lane
17. Turn signal indicators are required on all motor vehicles manufactured after the model year
18. 1971
19. 1948
20. 1969
21. **1959**
22. No Combination of vehicles other than a truck tractor-trailer combination may exceed
23. **65 feet**
24. 40 feet
25. 25 feet
26. 50 feet
27. The load on a truck may not extend over the rear of vehicle more than
28. 65 feet
29. **40 feet**
30. 25 feet
31. 50 feet
32. All buses, taxis’s, and other vehicles hauling passengers for hire or lease must carry a chemical type fire extinguisher of at least
33. one pint capacity
34. two quart capacity
35. **one quart capacity**
36. one gallon capacity
37. The greatest height ordinarily allowed by State law for vehicle including its load is
38. 12 feet
39. 12 feet, 6 inches
40. 13 feet, 6 inches
41. **14 feet**
42. When one truck is following another truck or vehicle, it may keep far enough back to allow how many vehicles to enter safely between them?
43. two vehicles
44. three vehicles
45. four vehicles
46. **one vehicle**
47. The greatest weight allowed by state law for any vehicle including the load is
48. 36,420
49. 48,000
50. **80,000**
51. 60,000
52. A slow moving vehicle emblem must be displayed only by
53. All commercial vehicles
54. Delivery trucks which occasionally drive under 25 mph
55. All road machinery driving under 25 mph
56. **Vehicles designed to be operated at speeds of 25 mph or less**
57. Which of the following vehicles are not required to have mud flaps?
58. Semi-trailers
59. Vehicles operated interstate
60. **Pole trailers**
61. Vehicles hauling livestock
62. The height from the ground for mounted reflectors must be at least?
63. **24 inches**
64. 30 inches
65. 18 inches
66. 12 inches
67. The greatest width ordinarily allowed by State law for a truck including its load is
68. 108 inches (9 feet)
69. 90 inches (7 ½ feet)
70. **102 inches (8 ½ feet)**
71. 84 inches (7 feet)
72. Registration papers are required to be in the possession of the drive or on the vehicle when operating
73. A taxicab
74. A motorcycle
75. **All trucks**
76. Any ambulance
77. No passenger vehicle may be coupled with more than
78. **One trailer**
79. Two trailers
80. Three trailers
81. Four trailers
82. When mud flaps are required on trucks or trailers, they must reach how close to the surface of the highway?
83. **8 inches**
84. 12 inches
85. 16 inches
86. 18 inches
87. Every bus or truck manufactured after model year 1959 must be equipped on the rear with
88. **Two stop lights**
89. One stop light
90. One red reflector
91. Two yellow reflectors
92. Which of the following vehicles must have mud flaps when operated on public roads?
93. All vehicles with registered gross weight of 30,500 pounds
94. All truck trailer combinations
95. **All vehicles with four or more tires on the rear axle except single truck tractors and pole trailers**
96. All commercial vehicles
97. When a truck breaks down on a highway in the daytime the driver should set out
98. Two yellow flags
99. Three flares
100. **Two approved red flags**
101. Three red reflectors
102. Which of the following vehicles are required by state law to stop at railroad grade crossings outside city limits where no traffic control device is in operation?
103. **Buses carrying passengers for hire**
104. Trucks hauling livestock for hire
105. Truck trailer combinations
106. Taxicabs
107. The length requirements of state law for vehicles or combinations of vehicles, including extensions over front and rear, do not apply
108. **Within city limits**
109. On farm to marker highways
110. On state highways
111. On U.S. highways
112. When one vehicle is towing another, the distance between the two must not be greater than
113. 10 feet
114. **15 feet**
115. 20 feet
116. 45 feet
117. The greatest length allowed by state law for a single motor vehicle other than a truck tractor is
118. 40 feet
119. 30 feet
120. 50 feet
121. **45 feet**
122. Every farm tractor manufactured after January 1. 1972 complies with State lighting laws by
123. **Have two head lamps**
124. Traveling on the shoulder of the road
125. Stopping upon approach of another vehicle
126. Having one white lantern that shows to both the front and rear
127. To find out the details about registering your particular vehicle you should consult
128. City police
129. **Tax collector and assessor**
130. Railroad commission
131. Sheriffs office
132. One purpose of requiring registration papers on trucks at all times is to show
133. **Weight of the truck empty and how much it is registered to haul**
134. Ownership of the truck
135. Weight of truck when loaded
136. Counties in which the truck may be operated
137. Clearance lights are required by State law for trucks or buses if the width is
138. 75 inches or more
139. 70 inches or more
140. **80 inches or more**
141. 65 inches or more
142. When a load extends more than four feet over the rear of a vehicle, what color flag must be attached to the extreme end of the extension of driving in the daytime?
143. Green
144. White
145. **Red**
146. Blue
147. Which of the following vehicles is required by State law to carry a chemical type fire extinguisher
148. Ordinary passenger care
149. Truck hauling household goods
150. Cattle truck
151. **Taxicab**
152. It is unlawful to operate any motor vehicle on a highway with
153. Tire chains on the wheels
154. **Flanges or lugs on the wheels**
155. More than 10 tires on the ground
156. More than two mud-grip tires
157. To operate on the highway a motor vehicle or trailer having metal tires and weighing 5.000 pounds or more you must
158. Drive in the daytime only
159. **Get a special permit from the Department of Transportation**
160. Get a Highway Patrol escort
161. Drive less than 20 mph
162. Clearance lamps mounted on the rear or on the side near the rear of a vehicle must be what color?
163. Amber
164. White
165. Green
166. **Red**
167. When towing another vehicle with a chain or cable, what color flag must be attached to the chain or cable?
168. Red
169. **White**
170. Blue
171. Yellow
172. When going downhill with a commercial vehicle, it is unlawful to
173. Shift to a lower gear
174. Remain in the same gear
175. Travel more than 25 mph
176. **Coast**
177. The first thing the driver of a disabled truck or bus should do is
178. Try to get the vehicle started
179. **Set out flares, reflectors, or flags**
180. Flag down a vehicle to tow you in
181. Go for help
182. To haul a load or move equipment that is wider, heavier, or longer than the law permits, you must
183. Drive after dark on little traveled roads
184. **Obtain a permit from the Department of Transportation**
185. Obtain a permit from the police
186. Request a Highway patrol escort
187. Before going down a steep grade with a commercial vehicle you should
188. Remain in the same gear
189. Never be traveling more than 5 mph
190. Shift to a higher gear
191. **Shift to a lower gear**
192. To prevent damage to the highway, it is unlawful to operate any motor vehicle with
193. Tire chains on the wheels
194. **Studs or spikes in the wheels**
195. More than 10 tires on the ground
196. More than two mud grip tires